Hello, Lingxiang user. Thank you for choosing Lingxiang new energy equipment

To ensure your quick use, please prepare well

There are two types of software for extracting files to the computer: one is USB communication cable driver, and the other is v30 platform software




1: Open the box and plug in the power, then turn on the machine

2; Clamp the positive and negative terminals of the battery correctly, and it will make a dripping sound. It is strictly prohibited to clamp high voltage, otherwise it will burn out

3: Connect the computer and plug the communication cable into the computer USB. The blue end of the communication cable should not be plugged into the computer incorrectly

4: For users who are familiar with computers, we will send you a complete installation package and watch a video to install it. First, install the communication cable driver, and then install the platform software

5: If the above cannot be installed by oneself, please contact Lingxiang's technical department. The above preparation work must be completed before proceeding

6: Just open the start icon inside the v30 platform software





Answer to the Use of the Boge Lingxiang V20 New Energy Battery Pack Charging and Discharging Capacity Balancing Internal Resistance Testing Intelligent Machine

Using the process, click on refresh port ->click on the correct port ->click on the left connection ->select the main function, intelligent/professional/or custom

Click on the channel - centralized or branching - click on input parameters - click on the right side to start

Preparation for machine startup before installation - Plug in communication cable or wireless module - Install v30 platform software or mobile phone on the computer - Install APP - After installation, connect the device. The intelligent function is convenient, and it will automatically recognize the battery charging voltage, discharge voltage, charging current, and discharge current. No need to adjust any item

What does 3.2/3.7 mean? 3.2v represents iron lithium battery, and 3.7v represents ternary battery

3.2/3.7 represents two types of battery platform voltage. The nominal voltage is not selected to be 3.7 and then charged to 3.7. How much capacity should be filled in? Fill in the actual battery capacity

Is there a problem with filling in the wrong information? No problem. The larger the capacity, the greater the charging and discharging current of the battery

Charging

Click to start the machine and start charging. When the battery is fully charged and stopped, select 3.2 to automatically charge it to 3.65V

If you select 3.7, it will automatically be fully charged to 4.2V. If the battery is completely dead before charging, the displayed capacity after charging is complete indicates

Accurate full charge and capacity discharge of the battery

Click to start the machine and start discharging the battery. After discharging, stop selecting 3.2 and automatically switch to 2.5V

If you select 3.7, it will automatically switch to 2.8V. If the battery is fully charged before discharge, the displayed capacity after discharge indicates accuracy

The battery releases its storage capacity and automatically performs a cycle to fully charge it. After discharging, it automatically fills and discharges again, and the last step of charging is precise. The battery's storage capacity is balanced with just one click

When balancing voltage is required, fill in the battery capacity and fill in the balancing voltage. After starting, the system will calculate the voltage for each channel

Automatically balancing to the set voltage value, even if the voltage is consistent and the current is 0, it will not immediately stop and multiple data calculations will be performed

To reach the stop condition, this function does not calculate capacity, does not enable balancing function, does not need to be filled in, even if filled in, it is useless

Professional functions are used by specific users to freely set charging termination discharge termination charging current discharge current, charging termination current, etc

Data facilitates user specific use

Can be freely set to allow the machine to charge and discharge as much V as possible, with functions such as cycling the charging and discharging data, and terminating the current indicates charging

How much does the current drop to after reaching the voltage? Stop and terminate the current at 0.5-1A, which is most suitable

It is also a set of 4 sub functions for charging and discharging cycles or equalization

Customization function: Customization function is used to quickly start the user's last set save data execution. The name can be set, the rest time can be set, and it can be customized

Yi Edit 3 sets of storage functions that can be set to charge any amount of V, put it in any amount of V, and cycle multiple times


